data_migration
Normal
/

ID_BATCH
Y
ID_BATCH
CHANNEL_ID
Y
CHANNEL_ID
TRANSNAME
Y
TRANSNAME
STATUS
Y
STATUS
LINES_READ
Y
LINES_READ
LINES_WRITTEN
Y
LINES_WRITTEN
LINES_UPDATED
Y
LINES_UPDATED
LINES_INPUT
Y
LINES_INPUT
LINES_OUTPUT
Y
LINES_OUTPUT
LINES_REJECTED
Y
LINES_REJECTED
ERRORS
Y
ERRORS
STARTDATE
Y
STARTDATE
ENDDATE
Y
ENDDATE
LOGDATE
Y
LOGDATE
DEPDATE
Y
DEPDATE
REPLAYDATE
Y
REPLAYDATE
LOG_FIELD
Y
LOG_FIELD
EXECUTING_SERVER
N
EXECUTING_SERVER
EXECUTING_USER
N
EXECUTING_USER
CLIENT
N
CLIENT

ID_BATCH
Y
ID_BATCH
SEQ_NR
Y
SEQ_NR
LOGDATE
Y
LOGDATE
TRANSNAME
Y
TRANSNAME
STEPNAME
Y
STEPNAME
STEP_COPY
Y
STEP_COPY
LINES_READ
Y
LINES_READ
LINES_WRITTEN
Y
LINES_WRITTEN
LINES_UPDATED
Y
LINES_UPDATED
LINES_INPUT
Y
LINES_INPUT
LINES_OUTPUT
Y
LINES_OUTPUT
LINES_REJECTED
Y
LINES_REJECTED
ERRORS
Y
ERRORS
INPUT_BUFFER_ROWS
Y
INPUT_BUFFER_ROWS
OUTPUT_BUFFER_ROWS
Y
OUTPUT_BUFFER_ROWS

ID_BATCH
Y
ID_BATCH
CHANNEL_ID
Y
CHANNEL_ID
LOG_DATE
Y
LOG_DATE
LOGGING_OBJECT_TYPE
Y
LOGGING_OBJECT_TYPE
OBJECT_NAME
Y
OBJECT_NAME
OBJECT_COPY
Y
OBJECT_COPY
REPOSITORY_DIRECTORY
Y
REPOSITORY_DIRECTORY
FILENAME
Y
FILENAME
OBJECT_ID
Y
OBJECT_ID
OBJECT_REVISION
Y
OBJECT_REVISION
PARENT_CHANNEL_ID
Y
PARENT_CHANNEL_ID
ROOT_CHANNEL_ID
Y
ROOT_CHANNEL_ID

ID_BATCH
Y
ID_BATCH
CHANNEL_ID
Y
CHANNEL_ID
LOG_DATE
Y
LOG_DATE
TRANSNAME
Y
TRANSNAME
STEPNAME
Y
STEPNAME
STEP_COPY
Y
STEP_COPY
LINES_READ
Y
LINES_READ
LINES_WRITTEN
Y
LINES_WRITTEN
LINES_UPDATED
Y
LINES_UPDATED
LINES_INPUT
Y
LINES_INPUT
LINES_OUTPUT
Y
LINES_OUTPUT
LINES_REJECTED
Y
LINES_REJECTED
ERRORS
Y
ERRORS
LOG_FIELD
N
LOG_FIELD

ID_BATCH
Y
ID_BATCH
CHANNEL_ID
Y
CHANNEL_ID
LOG_DATE
Y
LOG_DATE
METRICS_DATE
Y
METRICS_DATE
METRICS_CODE
Y
METRICS_CODE
METRICS_DESCRIPTION
Y
METRICS_DESCRIPTION
METRICS_SUBJECT
Y
METRICS_SUBJECT
METRICS_TYPE
Y
METRICS_TYPE
METRICS_VALUE
Y
METRICS_VALUE

0.0
0.0
10000
50
50
N
Y
50000
Y
N
1000
100
romote_host
localhost
8085
cluster
Encrypted 2be98afc86aa7f2e48818bd79ddc0ff89
Y
N
-
2021/06/27 17:25:19.192
-
2021/06/27 17:25:19.192
H4sIAAAAAAAAAAMAAAAAAAAAAAA=
N
111.198.10.15-11209pg
111.198.10.15
POSTGRESQL Native smartwell 11209 postgres Encrypted 2be98afc86aa7f2e48818bd79ddc0ff89 `FORCE_IDENTIFIERS_TO_LOWERCASE` N `FORCE_IDENTIFIERS_TO_UPPERCASE` N `IS_CLUSTERED` N `PORT_NUMBER` 11209 `PRESERVE_RESERVED_WORD_CASE` Y `QUOTE_ALL_FIELDS` N `SUPPORTS_BOOLEAN_DATA_TYPE` Y `SUPPORTS_TIMESTAMP_DATA_TYPE` Y `USE_POOLING` N
111.198.10.15-smartwell20
111.198.10.15
MYSQL JNDI MYSQL8_15_DB 11336 Encrypted `EXTRA_OPTION_MYSQL.characterEncoding` utf8 `EXTRA_OPTION_MYSQL.rewriteBatchedStatements` true `EXTRA_OPTION_MYSQL.useCompression` true `EXTRA_OPTION_MYSQL.useSSL` false `EXTRA_OPTION_MYSQL.useServerPrepStmts` false `FORCE_IDENTIFIERS_TO_LOWERCASE` N `FORCE_IDENTIFIERS_TO_UPPERCASE` N `IS_CLUSTERED` N `PORT_NUMBER` 11336 `PRESERVE_RESERVED_WORD_CASE` Y `QUOTE_ALL_FIELDS` N `STREAM_RESULTS` Y `SUPPORTS_BOOLEAN_DATA_TYPE` Y `SUPPORTS_TIMESTAMP_DATA_TYPE` Y `USE_POOLING` N
alarm_job
表输出
Y
alarm_level
alarm_level_save
Y
alarm_records
alarm_records_save
Y
alarm_rule
alarm_rule_save
Y
base_alarm_content_type
base_alarm_content_type_save
Y
base_device_models
base_device_models_save
Y
base_device_type
base_device_type_save
Y
base_sensor
base_sensor_save
Y
bus_concentrator
bus_concentrator_save
Y
bus_config
bus_config_save
Y
bus_dept_user
bus_dept_user_save
Y
bus_device
bus_device_save
Y
bus_device_concentrator
bus_device_concentrator_save
Y
bus_device_sensor
bus_device_sensor_save
Y
bus_device_well
bus_device_well_save
Y
bus_imei_iccid
bus_imei_iccid_save
Y
bus_nb_device
bus_nb_device_save
Y
bus_well_info
bus_well_info_save
Y
config_dept_permission
config_dept_permission_save
Y
config_nb_cucc
config_nb_cucc_save
Y
data_dig
data_dig_save
Y
data_gasliquid_gas
data_gasliquid_gas_save
Y
data_gasliquid_liquid
data_gasliquid_liquid_save
Y
data_harmful_gas
data_harmful_gas_save
Y
data_hydrant
data_hydrant_save
Y
data_liquid
data_liquid_save
Y
data_noise
data_noise_save
Y
data_temp_hum
data_temp_hum_save
Y
data_tube
data_tube_save
Y
data_wellcover
data_wellcover_save
Y
data_wellcover_loca
data_wellcover_loca_save
Y
data_wellplus
data_wellplus_save
Y
- alarm_job
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , JOBCODE , JOG_TYPE , WELL_CODE , DEVCODE , CREATE_TIME , JOB_STATUS , JOB_BELONG_TO , SHOULD_GET_TIME , GET_JOB_PERSON , GET_JOB_TIME , FIRST_STATE , FIRST_STATE_PHOTOS , CONFIRM_JOB_PERSON , CONFRIM_JOB_TIME , HANDLE_JOB_PERSON , SHOULD_HANDLE_TIME , HANDLE_JOB_TIME , HANDLE_MESSAGE , HANDLE_PHOTOS , FLOW , JOB_FLAG_DELAY , JOB_FLAG_1 FROM smartwell.alarm_job 0 N N N N Integer normal ID 15 0 表输入 ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal JOBCODE 32 -1 表输入 JOBCODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal JOG_TYPE 32 -1 表输入 JOG_TYPE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal WELL_CODE 32 -1 表输入 WELL_CODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DEVCODE 32 -1 表输入 DEVCODE . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal CREATE_TIME 0 -1 表输入 CREATE_TIME . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal JOB_STATUS 1 -1 表输入 JOB_STATUS . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal JOB_BELONG_TO 15 0 表输入 JOB_BELONG_TO ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal SHOULD_GET_TIME 0 -1 表输入 SHOULD_GET_TIME . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal GET_JOB_PERSON 15 0 表输入 GET_JOB_PERSON ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal GET_JOB_TIME 0 -1 表输入 GET_JOB_TIME . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal FIRST_STATE 255 -1 表输入 FIRST_STATE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal FIRST_STATE_PHOTOS 255 -1 表输入 FIRST_STATE_PHOTOS . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal CONFIRM_JOB_PERSON 15 0 表输入 CONFIRM_JOB_PERSON ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal CONFRIM_JOB_TIME 0 -1 表输入 CONFRIM_JOB_TIME . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal HANDLE_JOB_PERSON 15 0 表输入 HANDLE_JOB_PERSON ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal SHOULD_HANDLE_TIME 0 -1 表输入 SHOULD_HANDLE_TIME . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal HANDLE_JOB_TIME 0 -1 表输入 HANDLE_JOB_TIME . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal HANDLE_MESSAGE 21845 -1 表输入 HANDLE_MESSAGE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal HANDLE_PHOTOS 255 -1 表输入 HANDLE_PHOTOS . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal FLOW 21845 -1 表输入 FLOW . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal JOB_FLAG_DELAY 1 -1 表输入 JOB_FLAG_DELAY . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal JOB_FLAG_1 1 -1 表输入 JOB_FLAG_1 . , none N Y 0 N N N zh_CN Asia/Shanghai N 64 48 Y
- alarm_level
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , NAME , DEVICE_TYPE , LEVEL , LOW_VALUE , HIGH_VALUE , OPEN_ALARM , OPEN_JOB , TENANT_ID , TS FROM smartwell.alarm_level 0 N N N N Integer normal ID 15 0 alarm_job 2 ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal NAME 30 -1 alarm_job 2 NAME . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal DEVICE_TYPE 15 0 alarm_job 2 DEVICE_TYPE ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal LEVEL 9 0 alarm_job 2 LEVEL ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N Number normal LOW_VALUE -1 -1 alarm_job 2 LOW_VALUE ####0.0#########;-####0.0######### . , none N Y 0 N N N zh_CN Asia/Shanghai N Number normal HIGH_VALUE -1 -1 alarm_job 2 HIGH_VALUE ####0.0#########;-####0.0######### . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal OPEN_ALARM 1 -1 alarm_job 2 OPEN_ALARM . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal OPEN_JOB 1 -1 alarm_job 2 OPEN_JOB . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal TENANT_ID 15 0 alarm_job 2 TENANT_ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal TS 0 -1 alarm_job 2 TS . , none N Y 0 N N N zh_CN Asia/Shanghai N 64 112 Y
- alarm_level_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  alarm_level

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  NAME
  NAME
  DEVICE_TYPE
  DEVICE_TYPE
  LEVEL
  LEVEL
  LOW_VALUE
  LOW_VALUE
  HIGH_VALUE
  HIGH_VALUE
  OPEN_ALARM
  OPEN_ALARM
  OPEN_JOB
  OPEN_JOB
  TENANT_ID
  TENANT_ID
  TS
  TS
  176
  112
  Y
- alarm_records
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , DEVICE_ID , DEVCODE , WELL_CODE , ALARM_TYPE , ALARM_CONTENT , ALARM_VALUE , ALARM_LEVEL , ALARM_TIME , STATUS , JOB_ID , ALARM_MSG FROM smartwell.alarm_records 0 N N N N Integer normal ID 15 0 alarm_records ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal DEVICE_ID 15 0 alarm_records DEVICE_ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DEVCODE 32 -1 alarm_records DEVCODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal WELL_CODE 255 -1 alarm_records WELL_CODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal ALARM_TYPE 1 -1 alarm_records ALARM_TYPE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal ALARM_CONTENT 255 -1 alarm_records ALARM_CONTENT . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal ALARM_VALUE 255 -1 alarm_records ALARM_VALUE . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal ALARM_LEVEL 9 0 alarm_records ALARM_LEVEL ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal ALARM_TIME 0 -1 alarm_records ALARM_TIME . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal STATUS 1 -1 alarm_records STATUS . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal JOB_ID 15 0 alarm_records JOB_ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal ALARM_MSG 255 -1 alarm_records ALARM_MSG . , none N Y 0 N N N zh_CN Asia/Shanghai N 64 208 Y
- alarm_records_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  alarm_records

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  DEVICE_ID
  DEVICE_ID
  DEVCODE
  DEVCODE
  WELL_CODE
  WELL_CODE
  ALARM_TYPE
  ALARM_TYPE
  ALARM_CONTENT
  ALARM_CONTENT
  ALARM_VALUE
  ALARM_VALUE
  ALARM_LEVEL
  ALARM_LEVEL
  ALARM_TIME
  ALARM_TIME
  STATUS
  STATUS
  JOB_ID
  JOB_ID
  ALARM_MSG
  ALARM_MSG
  176
  208
  Y
- alarm_rule
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , DEVCODE , HIGHVALUE , LOWVALUE , OVERTIME , SALTATION , SENSORCODE , GRADE , TS , OPERATOR FROM smartwell.alarm_rule 0 N N N N Integer normal ID 15 0 alarm_rule ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DEVCODE 32 -1 alarm_rule DEVCODE . , none N Y 0 N N N zh_CN Asia/Shanghai N Number normal HIGHVALUE -1 -1 alarm_rule HIGHVALUE ####0.0#########;-####0.0######### . , none N Y 0 N N N zh_CN Asia/Shanghai N Number normal LOWVALUE -1 -1 alarm_rule LOWVALUE ####0.0#########;-####0.0######### . , none N Y 0 N N N zh_CN Asia/Shanghai N Number normal OVERTIME -1 -1 alarm_rule OVERTIME ####0.0#########;-####0.0######### . , none N Y 0 N N N zh_CN Asia/Shanghai N Number normal SALTATION -1 -1 alarm_rule SALTATION ####0.0#########;-####0.0######### . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal SENSORCODE 255 -1 alarm_rule SENSORCODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal GRADE 100 -1 alarm_rule GRADE . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal TS 0 -1 alarm_rule TS . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal OPERATOR 100 -1 alarm_rule OPERATOR . , none N Y 0 N N N zh_CN Asia/Shanghai N 64 272 Y
- alarm_rule_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  alarm_rule

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  DEVCODE
  DEVCODE
  HIGHVALUE
  HIGHVALUE
  LOWVALUE
  LOWVALUE
  OVERTIME
  OVERTIME
  SALTATION
  SALTATION
  SENSORCODE
  SENSORCODE
  GRADE
  GRADE
  TS
  TS
  OPERATOR
  OPERATOR
  176
  272
  Y
- base_alarm_content_type
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , ALARM_CONTENT , ALARM_TYPE , DEVICE_TYPE FROM smartwell.base_alarm_content_type 0 N N N N Integer normal ID 15 0 base_alarm_content_type ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal ALARM_CONTENT 255 -1 base_alarm_content_type ALARM_CONTENT . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal ALARM_TYPE 15 0 base_alarm_content_type ALARM_TYPE ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal DEVICE_TYPE 15 0 base_alarm_content_type DEVICE_TYPE ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N 32 352 Y
- base_alarm_content_type_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  base_alarm_content_type

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  ALARM_CONTENT
  ALARM_CONTENT
  ALARM_TYPE
  ALARM_TYPE
  DEVICE_TYPE
  DEVICE_TYPE
  192
  352
  Y
- base_device_models
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , MODEL_NAME , DEVICE_TYPE , COMMUNICATION FROM smartwell.base_device_models 0 N N N N Integer normal ID 15 0 base_device_models ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal MODEL_NAME 255 -1 base_device_models MODEL_NAME . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal DEVICE_TYPE 15 0 base_device_models DEVICE_TYPE ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal COMMUNICATION 100 -1 base_device_models COMMUNICATION . , none N Y 0 N N N zh_CN Asia/Shanghai N 368 48 Y
- base_device_models_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  base_device_models

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  MODEL_NAME
  MODEL_NAME
  DEVICE_TYPE
  DEVICE_TYPE
  COMMUNICATION
  COMMUNICATION
  512
  48
  Y
- base_device_type
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , TYPE_NAME , TYPE_DESCRIPTION , VALID , WATCH_TYPE , IS_NO_CONCENT FROM smartwell.base_device_type 0 N N N N Integer normal ID 15 0 base_device_type ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal TYPE_NAME 255 -1 base_device_type TYPE_NAME . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal TYPE_DESCRIPTION 255 -1 base_device_type TYPE_DESCRIPTION . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal VALID 1 -1 base_device_type VALID . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal WATCH_TYPE 100 -1 base_device_type WATCH_TYPE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal IS_NO_CONCENT 1 -1 base_device_type IS_NO_CONCENT . , none N Y 0 N N N zh_CN Asia/Shanghai N 368 112 Y
- base_device_type_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  base_device_type

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  TYPE_NAME
  TYPE_NAME
  TYPE_DESCRIPTION
  TYPE_DESCRIPTION
  VALID
  VALID
  WATCH_TYPE
  WATCH_TYPE
  IS_NO_CONCENT
  IS_NO_CONCENT
  512
  112
  Y
- base_sensor
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , SENSORCODE , ACTIVE , SENSORNAME , WATCH , DEVICE_TYPE FROM smartwell.base_sensor 0 N N N N Integer normal ID 15 0 base_sensor ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal SENSORCODE 255 -1 base_sensor SENSORCODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal ACTIVE 1 -1 base_sensor ACTIVE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal SENSORNAME 255 -1 base_sensor SENSORNAME . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal WATCH 255 -1 base_sensor WATCH . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal DEVICE_TYPE 9 0 base_sensor DEVICE_TYPE ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N 368 176 Y
- base_sensor_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  base_sensor

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  SENSORCODE
  SENSORCODE
  ACTIVE
  ACTIVE
  SENSORNAME
  SENSORNAME
  WATCH
  WATCH
  DEVICE_TYPE
  DEVICE_TYPE
  512
  176
  Y
- bus_concentrator
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , CONCENCODE , SIMID , DEPTID , `POSITION` , LAT , LNG , LAT_BAIDU , LNG_BAIDU , LAT_GAODE , LNG_GAODE , PHOTOS , STATUS , LASTTIME , VALID , SETUPDATE , TS , PHOTO FROM smartwell.bus_concentrator 0 N N N N Integer normal ID 15 0 bus_concentrator ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal CONCENCODE 255 -1 bus_concentrator CONCENCODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal SIMID 255 -1 bus_concentrator SIMID . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal DEPTID 15 0 bus_concentrator DEPTID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal POSITION 255 -1 bus_concentrator POSITION . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal LAT 255 -1 bus_concentrator LAT . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal LNG 255 -1 bus_concentrator LNG . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal LAT_BAIDU 255 -1 bus_concentrator LAT_BAIDU . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal LNG_BAIDU 255 -1 bus_concentrator LNG_BAIDU . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal LAT_GAODE 255 -1 bus_concentrator LAT_GAODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal LNG_GAODE 255 -1 bus_concentrator LNG_GAODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal PHOTOS 255 -1 bus_concentrator PHOTOS . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal STATUS 255 -1 bus_concentrator STATUS . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal LASTTIME 0 -1 bus_concentrator LASTTIME . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal VALID 2 -1 bus_concentrator VALID . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal SETUPDATE 0 -1 bus_concentrator SETUPDATE . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal TS 0 -1 bus_concentrator TS . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal PHOTO 255 -1 bus_concentrator PHOTO . , none N Y 0 N N N zh_CN Asia/Shanghai N 368 240 Y
- bus_concentrator_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  bus_concentrator

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  CONCENCODE
  CONCENCODE
  SIMID
  SIMID
  DEPTID
  DEPTID
  POSITION
  POSITION
  LAT
  LAT
  LNG
  LNG
  LAT_BAIDU
  LAT_BAIDU
  LNG_BAIDU
  LNG_BAIDU
  LAT_GAODE
  LAT_GAODE
  LNG_GAODE
  LNG_GAODE
  PHOTOS
  PHOTOS
  STATUS
  STATUS
  LASTTIME
  LASTTIME
  VALID
  VALID
  SETUPDATE
  SETUPDATE
  TS
  TS
  PHOTO
  PHOTO
  512
  240
  Y
- bus_config
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , DEVICE_ID , FRAMECONTENT , SENSORID , SENSORCODE , STATUS , ATTEMPTSMAX , ATTEMPTSCURRENT , SENDTIME , WRITETIME FROM smartwell.bus_config 0 N N N N Integer normal ID 15 0 bus_config ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal DEVICE_ID 15 0 bus_config DEVICE_ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal FRAMECONTENT 255 -1 bus_config FRAMECONTENT . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal SENSORID 255 -1 bus_config SENSORID . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal SENSORCODE 255 -1 bus_config SENSORCODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal STATUS 1 -1 bus_config STATUS . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal ATTEMPTSMAX 9 0 bus_config ATTEMPTSMAX ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal ATTEMPTSCURRENT 9 0 bus_config ATTEMPTSCURRENT ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal SENDTIME 0 -1 bus_config SENDTIME . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal WRITETIME 0 -1 bus_config WRITETIME . , none N Y 0 N N N zh_CN Asia/Shanghai N 368 304 Y
- bus_config_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  bus_config

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  DEVICE_ID
  DEVICE_ID
  FRAMECONTENT
  FRAMECONTENT
  SENSORID
  SENSORID
  SENSORCODE
  SENSORCODE
  STATUS
  STATUS
  ATTEMPTSMAX
  ATTEMPTSMAX
  ATTEMPTSCURRENT
  ATTEMPTSCURRENT
  SENDTIME
  SENDTIME
  WRITETIME
  WRITETIME
  512
  304
  Y
- bus_dept_user
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , DEPTID , USER , NUM FROM smartwell.bus_dept_user 0 N N N N Integer normal ID 15 0 bus_dept_user ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal DEPTID 15 0 bus_dept_user DEPTID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal USER 15 0 bus_dept_user USER ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal NUM 9 0 bus_dept_user NUM ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N 368 368 Y
- bus_dept_user_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  bus_dept_user

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  DEPTID
  DEPTID
  USER
  USER
  NUM
  NUM
  512
  368
  Y
- bus_device
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , DEVCODE , DEVICE_NAME , ONLINE_STATE , DEVICE_TYPE , VALID , INSTALL_DATE , LOGTIME , VERSION FROM smartwell.bus_device 0 N N N N Integer normal ID 15 0 bus_device ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DEVCODE 255 -1 bus_device DEVCODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DEVICE_NAME 255 -1 bus_device DEVICE_NAME . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal ONLINE_STATE 1 -1 bus_device ONLINE_STATE . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal DEVICE_TYPE 15 0 bus_device DEVICE_TYPE ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal VALID 1 -1 bus_device VALID . , none N Y 0 N N N zh_CN Asia/Shanghai N Date normal INSTALL_DATE -1 -1 bus_device INSTALL_DATE . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal LOGTIME 0 -1 bus_device LOGTIME . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal VERSION 15 0 bus_device VERSION ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N 384 464 Y
- bus_device_concentrator
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT DEVICE_ID , CONCEN_ID , STATUS , ACTIVE , TS FROM smartwell.bus_device_concentrator 0 N N N N Integer normal DEVICE_ID 15 0 bus_device_concentrator DEVICE_ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal CONCEN_ID 15 0 bus_device_concentrator CONCEN_ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N Boolean normal STATUS -1 -1 bus_device_concentrator STATUS . , none N Y 0 N N N zh_CN Asia/Shanghai N Boolean normal ACTIVE -1 -1 bus_device_concentrator ACTIVE . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal TS 0 -1 bus_device_concentrator TS . , none N Y 0 N N N zh_CN Asia/Shanghai N 400 544 Y
- bus_device_concentrator_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  bus_device_concentrator

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  DEVICE_ID
  DEVICE_ID
  CONCEN_ID
  CONCEN_ID
  STATUS
  STATUS
  ACTIVE
  ACTIVE
  TS
  TS
  544
  544
  Y
- bus_device_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  bus_device

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  DEVCODE
  DEVCODE
  DEVICE_NAME
  DEVICE_NAME
  ONLINE_STATE
  ONLINE_STATE
  DEVICE_TYPE
  DEVICE_TYPE
  VALID
  VALID
  INSTALL_DATE
  INSTALL_DATE
  LOGTIME
  LOGTIME
  VERSION
  VERSION
  528
  464
  Y
- bus_device_sensor
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , DEVICE_ID , SENSOR_ID , ACTIVE FROM smartwell.bus_device_sensor 0 N N N N Integer normal ID 15 0 bus_device_sensor ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal DEVICE_ID 15 0 bus_device_sensor DEVICE_ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal SENSOR_ID 15 0 bus_device_sensor SENSOR_ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal ACTIVE 1 -1 bus_device_sensor ACTIVE . , none N Y 0 N N N zh_CN Asia/Shanghai N 672 48 Y
- bus_device_sensor_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  bus_device_sensor

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  DEVICE_ID
  DEVICE_ID
  SENSOR_ID
  SENSOR_ID
  ACTIVE
  ACTIVE
  816
  48
  Y
- bus_device_well
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT DEVICE_ID , WELL_ID , TS , VALID FROM smartwell.bus_device_well 0 N N N N Integer normal DEVICE_ID 15 0 bus_device_well DEVICE_ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal WELL_ID 15 0 bus_device_well WELL_ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal TS 0 -1 bus_device_well TS . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal VALID 1 -1 bus_device_well VALID . , none N Y 0 N N N zh_CN Asia/Shanghai N 688 128 Y
- bus_device_well_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  bus_device_well

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  DEVICE_ID
  DEVICE_ID
  WELL_ID
  WELL_ID
  TS
  TS
  VALID
  VALID
  832
  128
  Y
- bus_imei_iccid
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , DEVCODE , IMEI , ICCID , LOGTIME FROM smartwell.bus_imei_iccid 0 N N N N Integer normal ID 15 0 bus_imei_iccid ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DEVCODE 255 -1 bus_imei_iccid DEVCODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal IMEI 255 -1 bus_imei_iccid IMEI . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal ICCID 255 -1 bus_imei_iccid ICCID . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal LOGTIME 0 -1 bus_imei_iccid LOGTIME . , none N Y 0 N N N zh_CN Asia/Shanghai N 688 224 Y
- bus_imei_iccid_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  bus_imei_iccid

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  DEVCODE
  DEVCODE
  IMEI
  IMEI
  ICCID
  ICCID
  LOGTIME
  LOGTIME
  832
  224
  Y
- bus_nb_device
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , NB_DEVICE_ID , DEVCODE , VERIFY_CODE , NODEID , TIMEOUT , NAME , MANUFACTURER_ID , MANUFACTURER_NAME , DEVICE_TYPE , MODEL , PROTOCAL_TYPE , IS_SECURE FROM smartwell.bus_nb_device 0 N N N N Integer normal ID 15 0 bus_nb_device ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal NB_DEVICE_ID 255 -1 bus_nb_device NB_DEVICE_ID . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DEVCODE 255 -1 bus_nb_device DEVCODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal VERIFY_CODE 255 -1 bus_nb_device VERIFY_CODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal NODEID 255 -1 bus_nb_device NODEID . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal TIMEOUT 9 0 bus_nb_device TIMEOUT ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal NAME 255 -1 bus_nb_device NAME . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal MANUFACTURER_ID 255 -1 bus_nb_device MANUFACTURER_ID . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal MANUFACTURER_NAME 255 -1 bus_nb_device MANUFACTURER_NAME . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DEVICE_TYPE 255 -1 bus_nb_device DEVICE_TYPE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal MODEL 255 -1 bus_nb_device MODEL . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal PROTOCAL_TYPE 255 -1 bus_nb_device PROTOCAL_TYPE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal IS_SECURE 255 -1 bus_nb_device IS_SECURE . , none N Y 0 N N N zh_CN Asia/Shanghai N 688 304 Y
- bus_nb_device_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  bus_nb_device

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  NB_DEVICE_ID
  NB_DEVICE_ID
  DEVCODE
  DEVCODE
  VERIFY_CODE
  VERIFY_CODE
  NODEID
  NODEID
  TIMEOUT
  TIMEOUT
  NAME
  NAME
  MANUFACTURER_ID
  MANUFACTURER_ID
  MANUFACTURER_NAME
  MANUFACTURER_NAME
  DEVICE_TYPE
  DEVICE_TYPE
  MODEL
  MODEL
  PROTOCAL_TYPE
  PROTOCAL_TYPE
  IS_SECURE
  IS_SECURE
  832
  304
  Y
- bus_well_info
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , WELL_CODE , WELL_NAME , DEEP , COORDINATE_X , COORDINATE_Y , LNG_BAIDU , LAT_BAIDU , LNG_GAODE , LAT_GAODE , AREA , `POSITION` , DEPTID , RESPONSIBLE_DEPT , PHOTOS , NOTES , WELL_TYPE , STAFF , TEL , TS , VALID , BFZT , WELL_FLAG_1 , WELL_FLAG_2 , WELL_FLAG_3 FROM smartwell.bus_well_info 0 N N N N Integer normal ID 15 0 bus_well_info ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal WELL_CODE 255 -1 bus_well_info WELL_CODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal WELL_NAME 255 -1 bus_well_info WELL_NAME . , none N Y 0 N N N zh_CN Asia/Shanghai N Number normal DEEP -1 -1 bus_well_info DEEP ####0.0#########;-####0.0######### . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal COORDINATE_X 255 -1 bus_well_info COORDINATE_X . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal COORDINATE_Y 255 -1 bus_well_info COORDINATE_Y . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal LNG_BAIDU 32 -1 bus_well_info LNG_BAIDU . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal LAT_BAIDU 255 -1 bus_well_info LAT_BAIDU . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal LNG_GAODE 255 -1 bus_well_info LNG_GAODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal LAT_GAODE 255 -1 bus_well_info LAT_GAODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal AREA 255 -1 bus_well_info AREA . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal POSITION 255 -1 bus_well_info POSITION . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DEPTID 32 -1 bus_well_info DEPTID . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal RESPONSIBLE_DEPT 15 0 bus_well_info RESPONSIBLE_DEPT ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal PHOTOS 500 -1 bus_well_info PHOTOS . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal NOTES 255 -1 bus_well_info NOTES . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal WELL_TYPE 255 -1 bus_well_info WELL_TYPE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal STAFF 32 -1 bus_well_info STAFF . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal TEL 32 -1 bus_well_info TEL . , none N Y 0 N N N zh_CN Asia/Shanghai N Date normal TS -1 -1 bus_well_info TS . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal VALID 1 -1 bus_well_info VALID . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal BFZT 1 -1 bus_well_info BFZT . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal WELL_FLAG_1 10 -1 bus_well_info WELL_FLAG_1 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal WELL_FLAG_2 10 -1 bus_well_info WELL_FLAG_2 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal WELL_FLAG_3 10 -1 bus_well_info WELL_FLAG_3 . , none N Y 0 N N N zh_CN Asia/Shanghai N 688 368 Y
- bus_well_info_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  bus_well_info

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  WELL_CODE
  WELL_CODE
  WELL_NAME
  WELL_NAME
  DEEP
  DEEP
  COORDINATE_X
  COORDINATE_X
  COORDINATE_Y
  COORDINATE_Y
  LNG_BAIDU
  LNG_BAIDU
  LAT_BAIDU
  LAT_BAIDU
  LNG_GAODE
  LNG_GAODE
  LAT_GAODE
  LAT_GAODE
  AREA
  AREA
  POSITION
  POSITION
  DEPTID
  DEPTID
  RESPONSIBLE_DEPT
  RESPONSIBLE_DEPT
  PHOTOS
  PHOTOS
  NOTES
  NOTES
  WELL_TYPE
  WELL_TYPE
  STAFF
  STAFF
  TEL
  TEL
  TS
  TS
  VALID
  VALID
  BFZT
  BFZT
  WELL_FLAG_1
  WELL_FLAG_1
  WELL_FLAG_2
  WELL_FLAG_2
  WELL_FLAG_3
  WELL_FLAG_3
  832
  368
  Y
- config_dept_permission
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , DEPTID , COMMUNICATION , WELL_TYPE , DEVICE_TYPE , AREA , MAP , LNG , LAT FROM smartwell.config_dept_permission 0 N N N N Integer normal ID 15 0 config_dept_permission ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal DEPTID 15 0 config_dept_permission DEPTID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal COMMUNICATION 255 -1 config_dept_permission COMMUNICATION . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal WELL_TYPE 255 -1 config_dept_permission WELL_TYPE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DEVICE_TYPE 255 -1 config_dept_permission DEVICE_TYPE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal AREA 255 -1 config_dept_permission AREA . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal MAP 1 -1 config_dept_permission MAP . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal LNG 255 -1 config_dept_permission LNG . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal LAT 255 -1 config_dept_permission LAT . , none N Y 0 N N N zh_CN Asia/Shanghai N 688 448 Y
- config_dept_permission_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  config_dept_permission

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  DEPTID
  DEPTID
  COMMUNICATION
  COMMUNICATION
  WELL_TYPE
  WELL_TYPE
  DEVICE_TYPE
  DEVICE_TYPE
  AREA
  AREA
  MAP
  MAP
  LNG
  LNG
  LAT
  LAT
  848
  448
  Y
- config_nb_cucc
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , DEPTID , BASE_URL , APPID , APPKEY , SUBSCRIBE_URL , APPNAME FROM smartwell.config_nb_cucc 0 N N N N Integer normal ID 9 0 config_nb_cucc ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N Integer normal DEPTID 15 0 config_nb_cucc DEPTID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal BASE_URL 255 -1 config_nb_cucc BASE_URL . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal APPID 255 -1 config_nb_cucc APPID . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal APPKEY 255 -1 config_nb_cucc APPKEY . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal SUBSCRIBE_URL 255 -1 config_nb_cucc SUBSCRIBE_URL . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal APPNAME 255 -1 config_nb_cucc APPNAME . , none N Y 0 N N N zh_CN Asia/Shanghai N 704 544 Y
- config_nb_cucc_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  config_nb_cucc

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  DEPTID
  DEPTID
  BASE_URL
  BASE_URL
  APPID
  APPID
  APPKEY
  APPKEY
  SUBSCRIBE_URL
  SUBSCRIBE_URL
  APPNAME
  APPNAME
  864
  544
  Y
- data_dig
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , WELL_CODE , DEVCODE , CELL , DDATA , FREQUENCY , DESCN , UPTIME , LOGTIME , PCI , RSRP , SNR FROM smartwell.data_dig 0 N N N N Integer normal ID 9 0 data_dig ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal WELL_CODE 32 -1 data_dig WELL_CODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DEVCODE 255 -1 data_dig DEVCODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal CELL 255 -1 data_dig CELL . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DDATA 255 -1 data_dig DDATA . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal FREQUENCY 255 -1 data_dig FREQUENCY . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DESCN 255 -1 data_dig DESCN . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal UPTIME 0 -1 data_dig UPTIME . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal LOGTIME 0 -1 data_dig LOGTIME . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal PCI 255 -1 data_dig PCI . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal RSRP 255 -1 data_dig RSRP . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal SNR 255 -1 data_dig SNR . , none N Y 0 N N N zh_CN Asia/Shanghai N 1033 57 Y
- data_dig_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  data_dig

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  WELL_CODE
  WELL_CODE
  DEVCODE
  DEVCODE
  CELL
  CELL
  DDATA
  DDATA
  FREQUENCY
  FREQUENCY
  DESCN
  DESCN
  UPTIME
  UPTIME
  LOGTIME
  LOGTIME
  PCI
  PCI
  RSRP
  RSRP
  SNR
  SNR
  1193
  57
  Y
- data_gasliquid_gas
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , WELL_CODE , DEVCODE , CELL , STRENGTH , DESCN , UPTIME , LOGTIME FROM smartwell.data_gasliquid_gas 0 N N N N Integer normal ID 15 0 data_gasliquid_gas ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal WELL_CODE 32 -1 data_gasliquid_gas WELL_CODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DEVCODE 255 -1 data_gasliquid_gas DEVCODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal CELL 255 -1 data_gasliquid_gas CELL . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal STRENGTH 255 -1 data_gasliquid_gas STRENGTH . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DESCN 255 -1 data_gasliquid_gas DESCN . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal UPTIME 0 -1 data_gasliquid_gas UPTIME . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal LOGTIME 0 -1 data_gasliquid_gas LOGTIME . , none N Y 0 N N N zh_CN Asia/Shanghai N 1024 128 Y
- data_gasliquid_gas_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  data_gasliquid_gas

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  WELL_CODE
  WELL_CODE
  DEVCODE
  DEVCODE
  CELL
  CELL
  STRENGTH
  STRENGTH
  DESCN
  DESCN
  UPTIME
  UPTIME
  LOGTIME
  LOGTIME
  1184
  128
  Y
- data_gasliquid_liquid
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , WELL_CODE , DEVCODE , CELL , LIQUIDDATA , DESCN , UPTIME , LOGTIME FROM smartwell.data_gasliquid_liquid 0 N N N N BigNumber normal ID 16 0 data_gasliquid_liquid ID ######0.0###################;-######0.0################### . none N Y 0 N N N zh_CN Asia/Shanghai N String normal WELL_CODE 32 -1 data_gasliquid_liquid WELL_CODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DEVCODE 255 -1 data_gasliquid_liquid DEVCODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal CELL 255 -1 data_gasliquid_liquid CELL . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal LIQUIDDATA 255 -1 data_gasliquid_liquid LIQUIDDATA . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DESCN 255 -1 data_gasliquid_liquid DESCN . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal UPTIME 0 -1 data_gasliquid_liquid UPTIME . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal LOGTIME 0 -1 data_gasliquid_liquid LOGTIME . , none N Y 0 N N N zh_CN Asia/Shanghai N 1024 208 Y
- data_gasliquid_liquid_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  data_gasliquid_liquid

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  WELL_CODE
  WELL_CODE
  DEVCODE
  DEVCODE
  CELL
  CELL
  LIQUIDDATA
  LIQUIDDATA
  DESCN
  DESCN
  UPTIME
  UPTIME
  LOGTIME
  LOGTIME
  1184
  208
  Y
- data_harmful_gas
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , WELL_CODE , DEVCODE , CO , CH4 , H2S , O2 , SWITCH , DESCN , UPTIME , LOGTIME , pci , rsrp , snr FROM smartwell.data_harmful_gas 0 N N N N Integer normal ID 9 0 data_harmful_gas ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal WELL_CODE 32 -1 data_harmful_gas WELL_CODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DEVCODE 255 -1 data_harmful_gas DEVCODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal CO 255 -1 data_harmful_gas CO . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal CH4 255 -1 data_harmful_gas CH4 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal H2S 255 -1 data_harmful_gas H2S . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal O2 255 -1 data_harmful_gas O2 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal SWITCH 1 -1 data_harmful_gas SWITCH . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DESCN 255 -1 data_harmful_gas DESCN . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal UPTIME 0 -1 data_harmful_gas UPTIME . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal LOGTIME 0 -1 data_harmful_gas LOGTIME . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal pci 255 -1 data_harmful_gas pci . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal rsrp 255 -1 data_harmful_gas rsrp . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal snr 255 -1 data_harmful_gas snr . , none N Y 0 N N N zh_CN Asia/Shanghai N 1024 304 Y
- data_harmful_gas_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  data_harmful_gas

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  WELL_CODE
  WELL_CODE
  DEVCODE
  DEVCODE
  CO
  CO
  CH4
  CH4
  H2S
  H2S
  O2
  O2
  SWITCH
  SWITCH
  DESCN
  DESCN
  UPTIME
  UPTIME
  LOGTIME
  LOGTIME
  pci
  pci
  rsrp
  rsrp
  snr
  snr
  1184
  304
  Y
- data_hydrant
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , WELL_CODE , DEVCODE , STATUS , DESCN , LOGTIME FROM smartwell.data_hydrant 0 N N N N Integer normal ID 9 0 data_hydrant ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal WELL_CODE 32 -1 data_hydrant WELL_CODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DEVCODE 255 -1 data_hydrant DEVCODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal STATUS 255 -1 data_hydrant STATUS . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DESCN 255 -1 data_hydrant DESCN . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal LOGTIME 0 -1 data_hydrant LOGTIME . , none N Y 0 N N N zh_CN Asia/Shanghai N 1024 384 Y
- data_hydrant_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  data_hydrant

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  WELL_CODE
  WELL_CODE
  DEVCODE
  DEVCODE
  STATUS
  STATUS
  DESCN
  DESCN
  LOGTIME
  LOGTIME
  1184
  384
  Y
- data_liquid
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , WELL_CODE , DEVCODE , LOGTIME , CELL , LIQUIDDATA , DESCN , UPTIME , pci , rsrp , snr FROM smartwell.data_liquid 0 N N N N BigNumber normal ID 16 0 data_liquid ID ######0.0###################;-######0.0################### . none N Y 0 N N N zh_CN Asia/Shanghai N String normal WELL_CODE 32 -1 data_liquid WELL_CODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DEVCODE 255 -1 data_liquid DEVCODE . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal LOGTIME 0 -1 data_liquid LOGTIME . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal CELL 255 -1 data_liquid CELL . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal LIQUIDDATA 255 -1 data_liquid LIQUIDDATA . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DESCN 255 -1 data_liquid DESCN . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal UPTIME 0 -1 data_liquid UPTIME . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal pci 255 -1 data_liquid pci . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal rsrp 255 -1 data_liquid rsrp . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal snr 255 -1 data_liquid snr . , none N Y 0 N N N zh_CN Asia/Shanghai N 1056 464 Y
- data_liquid_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  data_liquid

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  WELL_CODE
  WELL_CODE
  DEVCODE
  DEVCODE
  LOGTIME
  LOGTIME
  CELL
  CELL
  LIQUIDDATA
  LIQUIDDATA
  DESCN
  DESCN
  UPTIME
  UPTIME
  pci
  pci
  rsrp
  rsrp
  snr
  snr
  1216
  464
  Y
- data_noise
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , WELL_CODE , DEVCODE , CELL , DDATA , FREQUENCY , UPTIME , LOGTIME , pci , rsrp , snr , DESCN FROM smartwell.data_noise 0 N N N N Integer normal ID 9 0 data_noise ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal WELL_CODE 255 -1 data_noise WELL_CODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DEVCODE 255 -1 data_noise DEVCODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal CELL 255 -1 data_noise CELL . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DDATA 255 -1 data_noise DDATA . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal FREQUENCY 255 -1 data_noise FREQUENCY . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal UPTIME 0 -1 data_noise UPTIME . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal LOGTIME 0 -1 data_noise LOGTIME . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal pci 255 -1 data_noise pci . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal rsrp 255 -1 data_noise rsrp . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal snr 255 -1 data_noise snr . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DESCN 255 -1 data_noise DESCN . , none N Y 0 N N N zh_CN Asia/Shanghai N 1056 528 Y
- data_noise_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  data_noise

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  WELL_CODE
  WELL_CODE
  DEVCODE
  DEVCODE
  CELL
  CELL
  DDATA
  DDATA
  FREQUENCY
  FREQUENCY
  UPTIME
  UPTIME
  LOGTIME
  LOGTIME
  pci
  pci
  rsrp
  rsrp
  snr
  snr
  DESCN
  DESCN
  1216
  528
  Y
- data_temp_hum
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , WELL_CODE , DEVCODE , CELL , TEMPERATURE , HUMIDITY , DESCN , UPTIME , LOGTIME , pci , rsrp , snr FROM smartwell.data_temp_hum 0 N N N N Integer normal ID 9 0 data_temp_hum ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal WELL_CODE 32 -1 data_temp_hum WELL_CODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DEVCODE 255 -1 data_temp_hum DEVCODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal CELL 255 -1 data_temp_hum CELL . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal TEMPERATURE 255 -1 data_temp_hum TEMPERATURE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal HUMIDITY 255 -1 data_temp_hum HUMIDITY . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DESCN 255 -1 data_temp_hum DESCN . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal UPTIME 0 -1 data_temp_hum UPTIME . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal LOGTIME 0 -1 data_temp_hum LOGTIME . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal pci 255 -1 data_temp_hum pci . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal rsrp 255 -1 data_temp_hum rsrp . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal snr 255 -1 data_temp_hum snr . , none N Y 0 N N N zh_CN Asia/Shanghai N 47 445 Y
- data_temp_hum_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  data_temp_hum

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  WELL_CODE
  WELL_CODE
  DEVCODE
  DEVCODE
  CELL
  CELL
  TEMPERATURE
  TEMPERATURE
  HUMIDITY
  HUMIDITY
  DESCN
  DESCN
  UPTIME
  UPTIME
  LOGTIME
  LOGTIME
  pci
  pci
  rsrp
  rsrp
  snr
  snr
  207
  445
  Y
- data_tube
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , WELL_CODE , DEVCODE , CELL , STRENGTH , DESCN , UPTIME , LOGTIME , pci , rsrp , snr FROM smartwell.data_tube 0 N N N N BigNumber normal ID 16 0 data_tube ID ######0.0###################;-######0.0################### . none N Y 0 N N N zh_CN Asia/Shanghai N String normal WELL_CODE 32 -1 data_tube WELL_CODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DEVCODE 255 -1 data_tube DEVCODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal CELL 255 -1 data_tube CELL . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal STRENGTH 255 -1 data_tube STRENGTH . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DESCN 255 -1 data_tube DESCN . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal UPTIME 0 -1 data_tube UPTIME . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal LOGTIME 0 -1 data_tube LOGTIME . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal pci 255 -1 data_tube pci . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal rsrp 255 -1 data_tube rsrp . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal snr 255 -1 data_tube snr . , none N Y 0 N N N zh_CN Asia/Shanghai N 58 519 Y
- data_tube_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  data_tube

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  WELL_CODE
  WELL_CODE
  DEVCODE
  DEVCODE
  CELL
  CELL
  STRENGTH
  STRENGTH
  DESCN
  DESCN
  UPTIME
  UPTIME
  LOGTIME
  LOGTIME
  pci
  pci
  rsrp
  rsrp
  snr
  snr
  218
  519
  Y
- data_wellcover
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , WELL_CODE , DEVCODE , STATUS , DESCN , LOGTIME FROM smartwell.data_wellcover 0 N N N N Integer normal ID 15 0 data_wellcover ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal WELL_CODE 32 -1 data_wellcover WELL_CODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DEVCODE 255 -1 data_wellcover DEVCODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal STATUS 255 -1 data_wellcover STATUS . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DESCN 255 -1 data_wellcover DESCN . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal LOGTIME 0 -1 data_wellcover LOGTIME . , none N Y 0 N N N zh_CN Asia/Shanghai N 66 589 Y
- data_wellcover_loca
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , WELL_CODE , DEVCODE , CELL , LNG , LAT , DESCN , LOGTIME , UPTIME FROM smartwell.data_wellcover_loca 0 N N N N Integer normal ID 9 0 data_wellcover_loca ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal WELL_CODE 32 -1 data_wellcover_loca WELL_CODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DEVCODE 255 -1 data_wellcover_loca DEVCODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal CELL 255 -1 data_wellcover_loca CELL . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal LNG 255 -1 data_wellcover_loca LNG . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal LAT 255 -1 data_wellcover_loca LAT . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DESCN 255 -1 data_wellcover_loca DESCN . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal LOGTIME 0 -1 data_wellcover_loca LOGTIME . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal UPTIME 0 -1 data_wellcover_loca UPTIME . , none N Y 0 N N N zh_CN Asia/Shanghai N 88 671 Y
- data_wellcover_loca_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  data_wellcover_loca

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  WELL_CODE
  WELL_CODE
  DEVCODE
  DEVCODE
  CELL
  CELL
  LNG
  LNG
  LAT
  LAT
  DESCN
  DESCN
  LOGTIME
  LOGTIME
  UPTIME
  UPTIME
  248
  671
  Y
- data_wellcover_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  data_wellcover

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  WELL_CODE
  WELL_CODE
  DEVCODE
  DEVCODE
  STATUS
  STATUS
  DESCN
  DESCN
  LOGTIME
  LOGTIME
  226
  589
  Y
- data_wellplus
  TableInput Y 1 none 111.198.10.15-smartwell20 SELECT ID , WELL_CODE , DEVCODE , STATUS , DESCN , LOGTIME FROM smartwell.data_wellplus 0 N N N N Integer normal ID 15 0 data_wellplus ID ####0;-####0 . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal WELL_CODE 32 -1 data_wellplus WELL_CODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DEVCODE 255 -1 data_wellplus DEVCODE . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal STATUS 255 -1 data_wellplus STATUS . , none N Y 0 N N N zh_CN Asia/Shanghai N String normal DESCN 255 -1 data_wellplus DESCN . , none N Y 0 N N N zh_CN Asia/Shanghai N Timestamp normal LOGTIME 0 -1 data_wellplus LOGTIME . , none N Y 0 N N N zh_CN Asia/Shanghai N 424 663 Y
- data_wellplus_save
  TableOutput Y 1 none 111.198.10.15-11209pg

  data_wellplus

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  WELL_CODE
  WELL_CODE
  DEVCODE
  DEVCODE
  STATUS
  STATUS
  DESCN
  DESCN
  LOGTIME
  LOGTIME
  584
  663
  Y
- 表输出
  TableOutput Y 1 none 111.198.10.15-11209pg

  alarm_job

  1000
  N
  N
  Y
  Y
  N
  N
  Y
  N
  Y
  N
  ID
  ID
  JOBCODE
  JOBCODE
  JOG_TYPE
  JOG_TYPE
  WELL_CODE
  WELL_CODE
  DEVCODE
  DEVCODE
  CREATE_TIME
  CREATE_TIME
  JOB_STATUS
  JOB_STATUS
  JOB_BELONG_TO
  JOB_BELONG_TO
  SHOULD_GET_TIME
  SHOULD_GET_TIME
  GET_JOB_PERSON
  GET_JOB_PERSON
  GET_JOB_TIME
  GET_JOB_TIME
  FIRST_STATE
  FIRST_STATE
  FIRST_STATE_PHOTOS
  FIRST_STATE_PHOTOS
  CONFIRM_JOB_PERSON
  CONFIRM_JOB_PERSON
  CONFRIM_JOB_TIME
  CONFRIM_JOB_TIME
  HANDLE_JOB_PERSON
  HANDLE_JOB_PERSON
  SHOULD_HANDLE_TIME
  SHOULD_HANDLE_TIME
  HANDLE_JOB_TIME
  HANDLE_JOB_TIME
  HANDLE_MESSAGE
  HANDLE_MESSAGE
  HANDLE_PHOTOS
  HANDLE_PHOTOS
  FLOW
  FLOW
  JOB_FLAG_DELAY
  JOB_FLAG_DELAY
  JOB_FLAG_1
  JOB_FLAG_1
  176
  48
  Y
N